**Steel Door Maintenance**

* Apply a layer of lubricant or silicone on hinges (1-2 times per year)

**Maintenance windows**

* Apply a silicone lubricant on the gear mechanism of your windows
* Clean the base and the outer covering of your PVC windows
* Never use abrasive cleaner to clean them
* Check regularly the status of joint sealant on windows to not cause water infiltration (joint damaged)
* If there is condensation (internal fogging), decrease the humidity inside the house.

For better circulation, remove the nets, this way, the windows will be easier to dry

* Minimal maintenance (cleaning profiles, lubrication of moving parts and weather-

stripping) should be done periodically.